(footprint "QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm_ThermalVias_LargerViaHoles" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 6206B69C)
  (descr "QFN, 20 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/3553fc.pdf#page=34), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference "U5" (at 0 -2.82) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 09fb01d0-4379-4d3a-bb86-d7479dfbcbd6)
  )
  (fp_text value "TMC6300" (at 0 2.82) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 99877568-b776-4553-be84-ba0b8129b2f3)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 0.75 0.75) (thickness 0.11)))
    (tstamp 7da46d4f-4e29-4376-9cc1-dc06ab7b607f)
  )
  (fp_line (start -1.16 1.61) (end -1.61 1.61) (layer "F.SilkS") (width 0.12) (tstamp 02d2363e-13ac-4bc9-b788-c3bd9b3c2cc0))
  (fp_line (start 1.16 -1.61) (end 1.61 -1.61) (layer "F.SilkS") (width 0.12) (tstamp 226bb7ad-6a92-4a06-bf07-d3cf91d90ef4))
  (fp_line (start -1.16 -1.61) (end -1.61 -1.61) (layer "F.SilkS") (width 0.12) (tstamp 2ed2be97-c539-4432-b5e6-838cb195ec75))
  (fp_line (start 1.61 1.61) (end 1.61 1.16) (layer "F.SilkS") (width 0.12) (tstamp 32e5dc58-27f6-42ff-a8d1-9340712c40cd))
  (fp_line (start -1.61 1.61) (end -1.61 1.16) (layer "F.SilkS") (width 0.12) (tstamp 68a86649-753f-4e66-a66d-97805c215e10))
  (fp_line (start 1.16 1.61) (end 1.61 1.61) (layer "F.SilkS") (width 0.12) (tstamp d9871b3e-affe-4219-aa8a-f0a51c3a307a))
  (fp_line (start 1.61 -1.61) (end 1.61 -1.16) (layer "F.SilkS") (width 0.12) (tstamp f086b697-0a9e-4914-990c-48f238bdcece))
  (fp_line (start 2.12 -2.12) (end -2.12 -2.12) (layer "F.CrtYd") (width 0.05) (tstamp 0bbc8b4f-44c7-4db1-a6c8-96d12fc9292a))
  (fp_line (start 2.12 2.12) (end 2.12 -2.12) (layer "F.CrtYd") (width 0.05) (tstamp 12ad2516-6970-48c5-8c9c-069629bdec35))
  (fp_line (start -2.12 -2.12) (end -2.12 2.12) (layer "F.CrtYd") (width 0.05) (tstamp a929cf87-3d42-4cd5-8b28-da62e1b300f8))
  (fp_line (start -2.12 2.12) (end 2.12 2.12) (layer "F.CrtYd") (width 0.05) (tstamp dfa77c89-25b1-4ce8-9b88-9c49eb6dc06c))
  (fp_line (start 1.5 1.5) (end -1.5 1.5) (layer "F.Fab") (width 0.1) (tstamp 4178c85b-dc4a-4466-8048-fc6a0a913480))
  (fp_line (start -1.5 1.5) (end -1.5 -0.75) (layer "F.Fab") (width 0.1) (tstamp 452d421e-0bb5-476b-80b0-c7ce06d29651))
  (fp_line (start -0.75 -1.5) (end 1.5 -1.5) (layer "F.Fab") (width 0.1) (tstamp 544c73f2-9c88-45ac-88a3-9da0ae3c5792))
  (fp_line (start -1.5 -0.75) (end -0.75 -1.5) (layer "F.Fab") (width 0.1) (tstamp 81cca155-55c4-4ab1-b013-e3b5f9dc0a56))
  (fp_line (start 1.5 -1.5) (end 1.5 1.5) (layer "F.Fab") (width 0.1) (tstamp fa8556e1-7b2a-4964-9288-df2bda67b28a))
  (pad "" smd roundrect (at 0.41 -0.41) (size 0.6 0.6) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp 90039618-6cb2-48fc-9714-37f106589a31))
  (pad "" smd roundrect (at -0.41 0.41) (size 0.6 0.6) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp bae8ee43-d884-49c9-9951-cf1b278a0ffd))
  (pad "" smd roundrect (at 0.41 0.41) (size 0.6 0.6) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp cc85b9ee-6c1a-4f81-83ff-a14a33d11117))
  (pad "" smd roundrect (at -0.41 -0.41) (size 0.6 0.6) (layers "F.Paste") (roundrect_rratio 0.25) (tstamp e1949ff9-f274-4e4b-bf87-443cbf233870))
  (pad "1" smd roundrect (at -1.45 -0.8) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 936bea39-2e00-4426-8699-fddc8cf7772e))
  (pad "2" smd roundrect (at -1.45 -0.4) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 13409c13-b1cb-4dbe-9abf-833e4b3e996d))
  (pad "3" smd roundrect (at -1.45 0) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 31282874-aa96-46e0-ab62-93e27ad65a8b))
  (pad "4" smd roundrect (at -1.45 0.4) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp bd2b77be-f184-4168-a0aa-e77c2caa46d5))
  (pad "5" smd roundrect (at -1.45 0.8) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 8768400b-6391-4a9d-943d-f8d27252bf25))
  (pad "6" smd roundrect (at -0.8 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp fc8f867f-4aee-41df-b1d6-92be9369e5d4))
  (pad "7" smd roundrect (at -0.4 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 26f70200-7762-4b2e-b244-b851ff4801df))
  (pad "8" smd roundrect (at 0 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dd1060ed-1c92-4b29-b26e-543e96cc9b11))
  (pad "9" smd roundrect (at 0.4 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 18bb59da-bc32-44de-82d1-4245fa7638ba))
  (pad "10" smd roundrect (at 0.8 1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d5af8127-a260-46a4-bce0-033769a21f79))
  (pad "11" smd roundrect (at 1.45 0.8) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e7294b88-276a-4a01-a13d-abe2e8533986))
  (pad "12" smd roundrect (at 1.45 0.4) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp b5486e78-c82d-4079-9ea4-7f62fe8416c5))
  (pad "13" smd roundrect (at 1.45 0) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4c63cb92-e61b-44e6-bca8-8f9371dbc10e))
  (pad "14" smd roundrect (at 1.45 -0.4) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d6b4c760-c565-4d97-87dd-2d21bce2352f))
  (pad "15" smd roundrect (at 1.45 -0.8) (size 0.7 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 4e8214b6-910c-4756-9b35-4760379ddc2d))
  (pad "16" smd roundrect (at 0.8 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6c259065-d9e9-4c18-9011-f9f7231f5dda))
  (pad "17" smd roundrect (at 0.4 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp e926b924-479d-4be2-871f-73cd0ec74350))
  (pad "18" smd roundrect (at 0 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp ab3a9411-e49b-4cd3-939f-e22ee6dd7176))
  (pad "19" smd roundrect (at -0.4 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 6b169ff4-43a6-42c2-b316-633647f234df))
  (pad "20" smd roundrect (at -0.8 -1.45) (size 0.2 0.7) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp d8e192fa-0c96-412b-8389-9cda0a5c2b9e))
  (pad "PAD" thru_hole circle (at -0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2) (tstamp 2425433c-cf8c-42c8-9410-372b6126b83f))
  (pad "PAD" thru_hole circle (at 0.5 -0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2) (tstamp 307b0505-edb0-4296-bf4b-3346771976c3))
  (pad "PAD" smd rect (at 0 0) (size 4 4) (layers "B.Cu" "B.Mask")
    (zone_connect 2) (tstamp 4e7ad814-d93a-4ebc-a5a1-d6eea38ad88e))
  (pad "PAD" thru_hole circle (at 0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2) (tstamp 61b4b466-5770-4b4a-850b-70299bba4740))
  (pad "PAD" thru_hole circle (at -0.5 0.5) (size 0.6 0.6) (drill 0.3) (layers *.Cu)
    (zone_connect 2) (tstamp a3963e6c-8ba2-406c-af49-43c1d04e5561))
  (pad "PAD" smd rect (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp f954229e-7e7b-41ab-b6af-fc32e2286d33))
  (model "${KISYS3DMOD}/Package_DFN_QFN.3dshapes/UQFN-20-1EP_3x3mm_P0.4mm_EP1.85x1.85mm.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/UQFN-20-1EP_3x3mm_P0.4mm_EP1.85x1.85mm.step"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
