(module GC9A01Round1.28 (layer F.Cu) (tedit 622E4650)
  (attr smd)
  (fp_text reference REF** (at 4 1) (layer F.SilkS) hide
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value GC9A01Round1.28 (at 0 -0.5) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 0 -5.7) (end -3 -5.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 5.7) (end -6.5 5.7) (layer F.SilkS) (width 0.15))
  (fp_line (start -6.5 -6.4) (end -4.5 -6.4) (layer F.SilkS) (width 0.15))
  (fp_line (start -4.5 -6.4) (end -3 -5.7) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 -5.7) (end 0 -4.5) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 5.7) (end 0 4.5) (layer F.SilkS) (width 0.15))
  (fp_text user 1 (at 2 -4) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.12)))
  )
  (fp_text user 12 (at 2 4) (layer F.SilkS)
    (effects (font (size 0.8 0.8) (thickness 0.12)))
  )
  (pad 1 smd roundrect (at 0 -3.85) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at 0 -3.15) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at 0 -2.45) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 0 -1.75) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 0 -1.05) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 0 -0.35) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 7 smd roundrect (at 0 0.35) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 8 smd roundrect (at 0 1.05) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 9 smd roundrect (at 0 1.75) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 10 smd roundrect (at 0 2.45) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 11 smd roundrect (at 0 3.15) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 12 smd roundrect (at 0 3.85) (size 2 0.35) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KIPRJMOD}/../lib/LCD_GC9A01.3dshapes/TFT-Round-1.28.step
    (offset (xyz 10.9 0 -1.8))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 90))
  )
)
